; pioport.INF
;
; Win95 Installation file (.inf) for the Generic LAVA 8255-PIO PCI devices.
;
; (c) Copyright 2000 Lava Computer MFG Inc.
;

[Version]
Signature="$Windows 95$"
Class=Ports
ClassGuid= {4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%

;DriverVer=11:07 AM 6/12/00,5.00.2183.1

; Install class "Ports"
;----------------------------------------------------------
[ClassInstall]
AddReg=PortsClass.AddReg

[Manufacturer]
%Mfg%=Models

[DestinationDirs]
DefaultDestDir=11
DriversDestDir=11
WindowsDir=10

[PortsClass.AddReg]
HKR,,,,%PortsClassName%

[ClassInstall32.NT]
AddReg=PortsClass.NT.AddReg

[PortsClass.NT.AddReg]
HKR,,,,%PortsClassName%
HKR,,Icon,,"-23"
HKR,,Installer32,,"MsPorts.Dll,PortsClassInstaller"

[Models]
%PIOPCI.DeviceDesc%=PIOPort,PCI\VEN_1407&DEV_0400

[ControlFlags]
ExcludeFromSelect=PCI\VEN_1407&DEV_0400

;;;;;;;;;;;;;;;;;;;;;; PIO Port

[PIOPort]
LogConfig=lcp
Reboot



[SourceDisksNames]
1=%ID1%,,

[SourceDisksFiles]
lavmdmfx.bin=1


[lcp]
ConfigPriority=HARDRECONFIG
IOConfig=8@100-ffff%fff8(ffff::)


;  Strings Section
;----------------------------------------------------------
[Strings]
ID1="Lava Installation & Utilities Diskette"
PortsClassName="Ports (COM & LPT)"
Mfg="Lava Computer MFG Inc."
PIOPCI.DeviceDesc="Lava 8255 PIO PCI"
;; Driver start code
SERVICE_BOOT_START     = 0 ; Driver started by the operating system loader.
SERVICE_SYSTEM_START   = 1 ; Driver started during OS initialization.
SERVICE_AUTO_START     = 2 ; Driver started by the Service Control Manager during system startup.
SERVICE_DEMAND_START   = 3 ; Driver started on demand by the Service Control Manager.
SERVICE_DISABLED       = 4 ; Indicates a driver that cannot be started.
